<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>IO2  IO2 </text>
<text>IO3  IO3 </text>
<text>LL  UL</text>
<text>N/C</text>
<text>N/C</text>
<text>GND</text>
<text>VCC</text>
<text>     IO11</text>
<text>IO4  IO9 </text>
<text>LL  UL</text>
<text>IO18 IO10</text>
<text>IO7  IO8 </text>
<text>GND</text>
<text>VCC</text>
<text>IO28 IO28</text>
<text>IO29 IO29</text>
<text>LL  UL</text>
<text>IO30    </text>
<text>IO31    </text>
<text>GND</text>
<text>VCC</text>
<text>IO25 IO17</text>
<text>IO24 IO15</text>
<text>LL  UL</text>
<text>IO23 IO14</text>
<text>IO22 IO27</text>
<text>GND</text>
<text>VCC</text>
<text>MMH_RASPBERRY_PI</text>
<text>v1.0</text>
<text>VCC = 3.3V</text>
<text>NOTES</text>
<text>J4 REQUIRES P5 ON RPi</text>
<text>MakerMod</text>
<text>SPI</text>
<text>I2C1</text>
<text>I2C0</text>
</plain>
<libraries>
<library name="engunneer-helper">
<packages>
<package name="MAKERMOD-MAIN-LOGO-SILK">
</package>
<package name="MAKERMOD-LOGO-BACK">
<description>Designed to fit under a MM6x2RAF</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="raspberry">
<description>&lt;h1&gt;&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi Board&lt;/a&gt;&lt;/h1&gt;
&lt;h2&gt;Changelog&lt;/h2&gt;
&lt;ul&gt;
&lt;li&gt;2014-01-25: Added RasPi Model B Rev 2&lt;/li&gt;
&lt;li&gt;2012-01-29: Initial version from Jacques&lt;/li&gt;
&lt;/ul&gt;

&lt;h2&gt;Licence&lt;/h2&gt;
This library stands under the &lt;a href="http://www.ohwr.org/projects/cernohl/wiki"&gt;CERN Open Hardware Licence&lt;/a&gt;.

&lt;h2&gt;Authors:&lt;/h2&gt;
&lt;a href="http://www.steffenvogel.de"&gt;Steffen Vogel&lt;/a&gt;&lt;br&gt;
&lt;a href="http://www.raspberrypi.org/phpBB3/memberlist.php?mode=viewprofile&amp;u=9306"&gt;Jacques Lagnel&lt;/a&gt;
&lt;h2&gt;Links&lt;/h2&gt;
&lt;a href="http://www.raspberrypi.org/wp-content/uploads/2012/12/Raspberry-Pi-Mounting-Hole-Template.png"&gt;Mounting Holes&lt;/a&gt;&lt;br&gt;
&lt;a href="http://elinux.org/RPi_Low-level_peripherals"&gt;GPIO Description&lt;/a&gt;&lt;br&gt;
&lt;a href="http://openlab.com.au/wp-content/uploads/2013/04/Raspberry_Pi_Dimensions.png"&gt;Dimensions&lt;/a&gt;</description>
<packages>
<package name="RPI-B-V2-MINISHIELD">
</package>
</packages>
</library>
<library name="engunneer-connectors">
<packages>
<package name="2X6-RAF-MAKERMOD">
</package>
</packages>
</library>
<library name="engunneer-passive">
<packages>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Digikey 742C083 series</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="engunneer-helper" package="MAKERMOD-MAIN-LOGO-SILK" value="LOGO_MM_BOTH_SILK"/>
<element name="U$2" library="engunneer-helper" package="MAKERMOD-LOGO-BACK" value="LOGO_MM_BOX_BSILK"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U$3" library="raspberry" package="RPI-B-V2-MINISHIELD" value="RPI-B-V2MINISHIELD"/>
<element name="J2" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="R3" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R4" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="J1" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="R2" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="J3" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="R5" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R6" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="J4" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="R7" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R8" library="engunneer-passive" package="0603-ARV" value="200"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="P1_9"/>
<contactref element="U$3" pad="P1_6"/>
<contactref element="U$3" pad="P1_25"/>
<contactref element="U$3" pad="P6_2"/>
<contactref element="U$3" pad="P5_8"/>
<contactref element="U$3" pad="P1_14"/>
<contactref element="U$3" pad="P5_7"/>
<contactref element="U$3" pad="P1_20"/>
<contactref element="J2" pad="11"/>
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="11"/>
<contactref element="J1" pad="5"/>
<contactref element="J3" pad="11"/>
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="11"/>
<contactref element="J4" pad="5"/>
<contactref element="U$3" pad="P5_8"/>
<contactref element="U$3" pad="P1_9"/>
<contactref element="U$3" pad="P1_20"/>
<contactref element="U$3" pad="P6_2"/>
<contactref element="U$3" pad="P1_6"/>
<contactref element="U$3" pad="P1_14"/>
<contactref element="U$3" pad="P1_25"/>
<contactref element="U$3" pad="P5_7"/>
</signal>
<signal name="RESET">
<contactref element="U$3" pad="P6_1"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="6"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="6"/>
<contactref element="J3" pad="12"/>
<contactref element="J3" pad="6"/>
<contactref element="J4" pad="12"/>
<contactref element="J4" pad="6"/>
<contactref element="U$3" pad="P1_17"/>
<contactref element="U$3" pad="P1_1"/>
<contactref element="U$3" pad="P5_2"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="4"/>
<contactref element="R4" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="1"/>
<contactref element="R3" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="8"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="N$16">
<contactref element="R4" pad="6"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="N$17">
<contactref element="R3" pad="8"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="R3" pad="6"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="1">
<contactref element="J2" pad="2"/>
<contactref element="R3" pad="7"/>
</signal>
<signal name="2">
<contactref element="J2" pad="3"/>
<contactref element="R4" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="4"/>
<contactref element="R2" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="8"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="6"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="4">
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="J3" pad="4"/>
<contactref element="R6" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="J3" pad="1"/>
<contactref element="R5" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="8"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="R6" pad="6"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="8"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="6"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="5">
<contactref element="J3" pad="2"/>
<contactref element="R5" pad="7"/>
</signal>
<signal name="6">
<contactref element="J3" pad="3"/>
<contactref element="R6" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="J4" pad="4"/>
<contactref element="R8" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="J4" pad="1"/>
<contactref element="R7" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="R8" pad="8"/>
<contactref element="J4" pad="10"/>
</signal>
<signal name="N$22">
<contactref element="R8" pad="6"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="N$23">
<contactref element="R7" pad="8"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="N$24">
<contactref element="R7" pad="6"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="7">
<contactref element="J4" pad="2"/>
<contactref element="R7" pad="7"/>
</signal>
<signal name="8">
<contactref element="J4" pad="3"/>
<contactref element="R8" pad="5"/>
</signal>
<signal name="IO2">
<contactref element="U$3" pad="P1_3"/>
<contactref element="R2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="IO3">
<contactref element="U$3" pad="P1_5"/>
<contactref element="R2" pad="4"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="IO4">
<contactref element="U$3" pad="P1_7"/>
<contactref element="R4" pad="3"/>
</signal>
<signal name="IO7">
<contactref element="U$3" pad="P1_26"/>
<contactref element="R3" pad="3"/>
</signal>
<signal name="IO8">
<contactref element="U$3" pad="P1_24"/>
<contactref element="R3" pad="4"/>
</signal>
<signal name="IO9">
<contactref element="U$3" pad="P1_21"/>
<contactref element="R4" pad="4"/>
</signal>
<signal name="IO10">
<contactref element="U$3" pad="P1_19"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="IO11">
<contactref element="U$3" pad="P1_23"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="IO14">
<contactref element="U$3" pad="P1_8"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="IO15">
<contactref element="U$3" pad="P1_10"/>
<contactref element="R6" pad="4"/>
</signal>
<signal name="IO17">
<contactref element="U$3" pad="P1_11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="IO18">
<contactref element="U$3" pad="P1_12"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IO22">
<contactref element="U$3" pad="P1_15"/>
<contactref element="R5" pad="3"/>
</signal>
<signal name="IO23">
<contactref element="U$3" pad="P1_16"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="IO24">
<contactref element="U$3" pad="P1_18"/>
<contactref element="R6" pad="3"/>
</signal>
<signal name="IO25">
<contactref element="U$3" pad="P1_22"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="IO27">
<contactref element="U$3" pad="P1_13"/>
<contactref element="R5" pad="4"/>
</signal>
<signal name="IO28">
<contactref element="U$3" pad="P5_3"/>
<contactref element="R8" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="IO29">
<contactref element="U$3" pad="P5_4"/>
<contactref element="R8" pad="4"/>
<contactref element="R8" pad="3"/>
</signal>
<signal name="IO30">
<contactref element="U$3" pad="P5_5"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="IO31">
<contactref element="U$3" pad="P5_6"/>
<contactref element="R7" pad="3"/>
</signal>
<signal name="N$46">
<contactref element="U$3" pad="P1_2"/>
<contactref element="U$3" pad="P1_4"/>
<contactref element="U$3" pad="P5_1"/>
</signal>
<signal name="N$33">
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
