<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="59.055" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="65.405" y2="0" width="0" layer="20"/>
<wire x1="65.405" y1="0" x2="66.04" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="66.04" y1="0.635" x2="66.04" y2="59.055" width="0" layer="20"/>
<wire x1="66.04" y1="59.055" x2="65.405" y2="59.69" width="0" layer="20" curve="90"/>
<wire x1="65.405" y1="59.69" x2="0.635" y2="59.69" width="0" layer="20"/>
<wire x1="0.635" y1="59.69" x2="0" y2="59.055" width="0" layer="20" curve="90"/>
<text>MMH_TEENSY_3.1</text>
<text>MakerMod</text>
<text>v1.0</text>
<text>D6  D14</text>
<text>D5  D0 </text>
<text>D4  D1 </text>
<text>D3  D2 </text>
<text>LL  UL </text>
<text>GND</text>
<text>VCC</text>
<text>D17    </text>
<text>D16 D7 </text>
<text>    D8 </text>
<text>       </text>
<text>LL  UL </text>
<text>GND</text>
<text>VCC</text>
<text>    D22</text>
<text>    D23</text>
<text>D19 D19</text>
<text>D18 D18</text>
<text>GND</text>
<text>VCC</text>
<text>UL  LL </text>
<text>D10 D9 </text>
<text>D11 D20</text>
<text>D12 D21</text>
<text>D13 D15</text>
<text>GND</text>
<text>VCC</text>
<text>UL  LL </text>
<text>D24 D32</text>
<text>D25 D33</text>
<text>A14 A12</text>
<text>AR  A13</text>
<text>UL  LL </text>
<text>D30 D29</text>
<text>D31 D28</text>
<text>D26 A10</text>
<text>D27 A11</text>
<text>UL  LL </text>
<text>SER1</text>
<text>I2CALT</text>
<text>SER3</text>
<text>I2C</text>
<text>SPI</text>
<text>SER2ALT</text>
<text>VCC = 3.3V</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>NOTES</text>
<text>A14 T3.1 ONLY</text>
<text>*=ALSO ANALOG</text>
<text>REQUIRES SMD HEADER ON TEENSY</text>
</plain>
<libraries>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1_ALLPINS">
</package>
</packages>
</library>
<library name="engunneer-connectors">
<packages>
<package name="2X6-RAF-MAKERMOD">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="engunneer-helper">
<packages>
<package name="MAKERMOD-MAIN-LOGO-MM-SILK">
</package>
<package name="MAKERMOD-LOGO-BACK">
<description>Designed to fit under a MM6x2RAF</description>
</package>
<package name="MAKERMOD-MAIN-TEXT-SILK">
</package>
</packages>
</library>
<library name="engunneer-passive">
<packages>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Digikey 742C083 series</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_ALLPINS" value="TEENSY_3.1_ALL_PINS_AND_PADS"/>
<element name="J1" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="J2" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="J3" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="J4" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="J5" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="J6" library="engunneer-connectors" package="2X6-RAF-MAKERMOD" value="MM6X2RAFEMALE">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U$2" library="engunneer-helper" package="MAKERMOD-MAIN-LOGO-MM-SILK" value="LOGO_MM_LOGO_SILK"/>
<element name="U$3" library="engunneer-helper" package="MAKERMOD-LOGO-BACK" value="LOGO_MM_BOX_BSILK"/>
<element name="U$4" library="engunneer-helper" package="MAKERMOD-MAIN-TEXT-SILK" value="LOGO_MM_TEXT_SILK"/>
<element name="R1" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R2" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R3" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R4" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R5" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R6" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R7" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R8" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R9" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R10" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R11" library="engunneer-passive" package="0603-ARV" value="200"/>
<element name="R12" library="engunneer-passive" package="0603-ARV" value="200"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="J5" pad="11"/>
<contactref element="J5" pad="5"/>
<contactref element="J6" pad="5"/>
<contactref element="J6" pad="11"/>
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="11"/>
<contactref element="J3" pad="11"/>
<contactref element="J3" pad="5"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="11"/>
<contactref element="J2" pad="5"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="AGND"/>
</signal>
<signal name="VBAT">
<contactref element="U$1" pad="VBAT"/>
</signal>
<signal name="VUSB">
<contactref element="U$1" pad="VUSB"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="6"/>
<contactref element="J5" pad="6"/>
<contactref element="J5" pad="12"/>
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="12"/>
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="12"/>
<contactref element="J3" pad="12"/>
<contactref element="J3" pad="6"/>
<contactref element="U$1" pad="3.3V2"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="U$1" pad="3.3V1"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="AREF">
<contactref element="U$1" pad="AREF"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="A14">
<contactref element="U$1" pad="A14"/>
<contactref element="R12" pad="4"/>
</signal>
<signal name="A13">
<contactref element="U$1" pad="A13"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="A12">
<contactref element="U$1" pad="A12"/>
<contactref element="R12" pad="3"/>
</signal>
<signal name="A11">
<contactref element="U$1" pad="A11"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="A10">
<contactref element="U$1" pad="A10"/>
<contactref element="R10" pad="3"/>
</signal>
<signal name="D0">
<contactref element="U$1" pad="0"/>
<contactref element="R2" pad="4"/>
</signal>
<signal name="D1">
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="2"/>
<contactref element="R1" pad="4"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="3"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="5"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="7"/>
<contactref element="R4" pad="4"/>
</signal>
<signal name="D8">
<contactref element="U$1" pad="8"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D9">
<contactref element="U$1" pad="9"/>
<contactref element="R7" pad="3"/>
</signal>
<signal name="D10">
<contactref element="U$1" pad="10"/>
<contactref element="R7" pad="4"/>
</signal>
<signal name="D11">
<contactref element="U$1" pad="11"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D12">
<contactref element="U$1" pad="12"/>
<contactref element="R8" pad="4"/>
</signal>
<signal name="D13">
<contactref element="U$1" pad="13"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="D14">
<contactref element="U$1" pad="14/A0"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D15">
<contactref element="U$1" pad="15/A1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="D16">
<contactref element="U$1" pad="16/A2"/>
<contactref element="R4" pad="3"/>
</signal>
<signal name="D17">
<contactref element="U$1" pad="17/A3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="D18">
<contactref element="U$1" pad="18/A4"/>
<contactref element="R6" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D19">
<contactref element="U$1" pad="19/A5"/>
<contactref element="R6" pad="3"/>
<contactref element="R6" pad="4"/>
</signal>
<signal name="D20">
<contactref element="U$1" pad="20/A6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="D21">
<contactref element="U$1" pad="21/A7"/>
<contactref element="R8" pad="3"/>
</signal>
<signal name="D22">
<contactref element="U$1" pad="22/A8"/>
<contactref element="R5" pad="3"/>
</signal>
<signal name="D23">
<contactref element="U$1" pad="23/A9"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="D24">
<contactref element="U$1" pad="24"/>
<contactref element="R11" pad="4"/>
</signal>
<signal name="D33">
<contactref element="U$1" pad="33"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="D32">
<contactref element="U$1" pad="32"/>
<contactref element="R11" pad="3"/>
</signal>
<signal name="D31">
<contactref element="U$1" pad="31"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="D30">
<contactref element="U$1" pad="30"/>
<contactref element="R9" pad="4"/>
</signal>
<signal name="D29">
<contactref element="U$1" pad="29"/>
<contactref element="R9" pad="3"/>
</signal>
<signal name="D28">
<contactref element="U$1" pad="28"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="D27">
<contactref element="U$1" pad="27"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="D26">
<contactref element="U$1" pad="26"/>
<contactref element="R10" pad="4"/>
</signal>
<signal name="D25">
<contactref element="U$1" pad="25"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="4"/>
<contactref element="R4" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="1"/>
<contactref element="R3" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="7"/>
<contactref element="R1" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="8"/>
<contactref element="R1" pad="8"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="9"/>
<contactref element="R2" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="10"/>
<contactref element="R2" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="J2" pad="10"/>
<contactref element="R4" pad="8"/>
</signal>
<signal name="N$16">
<contactref element="J2" pad="9"/>
<contactref element="R4" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="J2" pad="8"/>
<contactref element="R3" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="J2" pad="7"/>
<contactref element="R3" pad="6"/>
</signal>
<signal name="1">
<contactref element="J2" pad="2"/>
<contactref element="R3" pad="7"/>
</signal>
<signal name="2">
<contactref element="J2" pad="3"/>
<contactref element="R4" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="R3" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="R4" pad="2"/>
</signal>
<signal name="24">
<contactref element="J5" pad="1"/>
<contactref element="R9" pad="5"/>
</signal>
<signal name="23">
<contactref element="J5" pad="2"/>
<contactref element="R9" pad="7"/>
</signal>
<signal name="22">
<contactref element="J5" pad="3"/>
<contactref element="R10" pad="5"/>
</signal>
<signal name="21">
<contactref element="J5" pad="4"/>
<contactref element="R10" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="J5" pad="7"/>
<contactref element="R9" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="J5" pad="8"/>
<contactref element="R9" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="J5" pad="9"/>
<contactref element="R10" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="J5" pad="10"/>
<contactref element="R10" pad="8"/>
</signal>
<signal name="N$25">
<contactref element="J6" pad="4"/>
<contactref element="R12" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="J6" pad="3"/>
<contactref element="R12" pad="5"/>
</signal>
<signal name="N$27">
<contactref element="J6" pad="2"/>
<contactref element="R11" pad="7"/>
</signal>
<signal name="N$28">
<contactref element="J6" pad="1"/>
<contactref element="R11" pad="5"/>
</signal>
<signal name="N$29">
<contactref element="J6" pad="10"/>
<contactref element="R12" pad="8"/>
</signal>
<signal name="N$30">
<contactref element="J6" pad="9"/>
<contactref element="R12" pad="6"/>
</signal>
<signal name="N$31">
<contactref element="J6" pad="8"/>
<contactref element="R11" pad="8"/>
</signal>
<signal name="N$32">
<contactref element="J6" pad="7"/>
<contactref element="R11" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="J3" pad="7"/>
<contactref element="R5" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="J3" pad="8"/>
<contactref element="R5" pad="8"/>
</signal>
<signal name="N$35">
<contactref element="J3" pad="9"/>
<contactref element="R6" pad="6"/>
</signal>
<signal name="N$36">
<contactref element="J3" pad="10"/>
<contactref element="R6" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="J3" pad="1"/>
<contactref element="R5" pad="5"/>
</signal>
<signal name="N$38">
<contactref element="J3" pad="2"/>
<contactref element="R5" pad="7"/>
</signal>
<signal name="N$39">
<contactref element="J3" pad="3"/>
<contactref element="R6" pad="5"/>
</signal>
<signal name="N$40">
<contactref element="J3" pad="4"/>
<contactref element="R6" pad="7"/>
</signal>
<signal name="N$41">
<contactref element="J4" pad="1"/>
<contactref element="R7" pad="5"/>
</signal>
<signal name="N$42">
<contactref element="J4" pad="2"/>
<contactref element="R7" pad="7"/>
</signal>
<signal name="N$43">
<contactref element="J4" pad="3"/>
<contactref element="R8" pad="5"/>
</signal>
<signal name="N$44">
<contactref element="J4" pad="4"/>
<contactref element="R8" pad="7"/>
</signal>
<signal name="N$45">
<contactref element="J4" pad="10"/>
<contactref element="R8" pad="8"/>
</signal>
<signal name="N$46">
<contactref element="J4" pad="9"/>
<contactref element="R8" pad="6"/>
</signal>
<signal name="N$47">
<contactref element="J4" pad="8"/>
<contactref element="R7" pad="8"/>
</signal>
<signal name="N$48">
<contactref element="R7" pad="6"/>
<contactref element="J4" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
